iCarsoft ProfessionalMulti-system Auto DiagnosticTool POR V2.0 for Porsche, the Update version for iCarsoft POR II.

iCarsoft POR V2.0 is a Professional and powerful vehicle fault diagnosis tool developed by iCarsoft Technology Inc. With a 4.0” TFT LCD and unique diagnostic software, it features full ECU diagnosis of single vehicle brand and test modes mainly include: CANBUS, ISO9141, KWP2000, and J1850etc.Itenables technicians to accurately diagnose complex problems.

Based on POR II, more functions are added to POR V2.0:
ABS Bleeding
Injector Programming
BMS reset
Battery Voltage Test
Data Print

Notice:
iCarsoft POR V2.0 scanners just work on Porschewith OBD II protocol,
if your vehicle were produced before year2005 or after year 2016, please kindly confirm with us about the compatibility before purchasing !
If you want to test some specific functions, please also kindly confirm with us before purchasing, thank you !

Product Features:
1. iCarsoft POR V2.0 can do it all-reads and clears trouble codes on most of the systems such as engine, transmission, ABS and airbag etc.
2. Applies to the single Brand of most models of Porsche which equipped with OBDII-16 DLC
3. Support OBDII/EOBD Ten Modes of Operation
4. Full System Diagnosis
5. Read &Clear DTC
6. Read Live Data 
7. Support special functions: Oil Service Reset, EPB Reset, DPF reset, SAS Reset, ETCs reset, BMS Reset, ABS Bleeding and Injector Programming
8. Support Data Review
9. The Print Data function allows you printing out diagnostic data recorded by the scan tool or customized test reports.
10. Battery test allows you getting the Voltage of battery with OBD port by the scan tool when the engine starts.
11. DTC Library to lookup when user is operating this tool.
12. Easy To Use With Silicone Keys
13. Full Speed Upgrade Via USB2.0
14. 4.0″TFT LCD, 480*320 Pixels
15. Multi-language: English, German, Dutch, Spanish, French.

Special functions:
*** Varies across year and model ***
Oil Service Reset Function
The POR V2.0 allow you to reset OilService in a click of a button on supported vehicles. On vehicles where a manual reset is required, the tool will guide you through the full process step-by-step.

 EPB Reset Function:
This electric parking brake (EPB) function has a multitude of uses to maintain the electronic braking systemssafelyandeffectively. 
The applications include deactivating/activating the brake control system, assisting with brake fluid control, brake diagnostics, opening and closing brake pads, setting brakes after disc or pad replacement and also reading and clearing EPB/SBC trouble codes. It is also capable of retrieving Fault Codes information from the ECU.
DPF Regeneration or Replacement
Carry out a forced Diesel Particulate Filter (DPF) Regeneration on supported vehicles - this MUST be done by trained personnel. Required when the DPF filter blockage reaches levels where passive or active regeneration is unable to burn off the excess soot. 
SAS Reset Function
The Steering Angle Sensor (SAS) is used to measure the angle of the steering wheel and the speed at which it is being turned. The signal is mainly used by the ABS System as part of it's stability control function but also by other systems such as ride level control and adaptive lighting. A problem with the SAS Signal will cause a fault with any of the systems that use the signal directly, or indirectly.
If the Steering Angle Sensor (SAS) needs to be changed, many vehicles require the new sensor to be calibrated. The iCarsoft POR V2.0 will allow you to carry out steering angle re-calibration on supported models.
ETCs Reset Function
Electronic Throttle Control system (ETC) relearns the throttle valve control value while clear or replace the throttle valve.
BMS Reset Function
Battery Management System (BMS), registers new battery to the BMS while battery replacement.
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ABS Bleeding, release the air to restore ABS Brake sensitivity, or relearn while ABS replaced.

Injector Programming
Injector coding, relearn the injector control parameter while the injector renewed or replaced

POR V2.0 vehicle coverage of Porsche:
(If your vehicles are before 2004 year, please make sure your vehicles are OBDII compliant firstly)
Boxster – 981, 982,986, 987
Cayman – 981, 987
Cayenne – 955, 957, 958
911 – 991, 996, 997
Carrera GT - 980
Panamera – 970
GT2 (996)
GT3 (996)
Macan

*Please Note* - Scanner is NOT compatible with the (986) Boxster and the (996) 911 for Airbag and ABS diagnosis


SPCIFICATIONS:
Display: 4.0″TFT LCD, 480*320 Pixels
Operation Temperature: 0°C ~ 50°C
Storage Temperature: -20°C ~ 70°C
Operating PORtage: 9 ~ 18V
Operating Current: 150mA@12V(Typical)
Power Consumption: 1.8W(Typical)
Dimension: 206*104.1*32.6 mm (L x W x H)

CONTENTS:
POR V2.0 Main Unit
Main Cable
Data Cable
TF Card
User Manual
Nylon carry case


